

**Manufacturing Process**

Arrival of the wine at PM

According organic regulations

(for foreign wines EU-law applies)

↓

Sensoric evaluation and

full analysis at our wine laboratory

with full documentation

↓

Unloading into our stainless steel tanks

↓

Filtration

↓

Blending

↓

Final Filtration,

blend-analysis, sensoric evaluation

with full documentation

↓

Bottling on a fully automatic bottling line

- with add. membrane filtration before filling

- with cork closures and labelling

- with check on filling level by light stream

↓

Packing / Delivery